[bookmark: br1] 
Reference Material
This certificate  is designed in accordance  with ISO 17034  and ISO Guide  31. This reference  material (RM) was designed,produced
and verified  in accordance with ISO/IEC  17025, ISO  17034 and a registered  quality management  system ISO 9001.
Product Name  16 PAHs Mix in Acetonitrile,200µg/mL 

Part Number
Expiry Date
B64289
Lot Number
Storage
O21IB229482
2025-Jul-14
(2-8)°C,Keep in the shade 
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Intended Use
This RM is intended  for use in a  laboratory as a calibration  and quality control  standard or in method  development  for analytical
techniques.
Uncertainty
The certified  value(s) and uncertainty(ies)  are determined  in accordance  with ISO 17034 with  an 95% confidence  level (k=2).
Uncertainty is  based on the Total  Combined Uncertainty,  including uncertainties  of preparation,  purity of neat materials,
homogeneity,  stability testing.
Traceability
The balances  used for gravimetric  measurements are  calibrated with weights  traceable to the  national standards.  The calibration of
the balances  is verified annually  by an external accredited  calibration service.  This analysis method  has been verified  using an
approach consistent  with ISO 17034:2016  & ISO 17025:2017.
Homogeneity
Random replicate  samples of the  final packaged RM  have been analysed  to prove homogeneity  consistent with ISO  17034.
Storage
The RM should  be stored in the original  sealed bottle  at the indicated temperature.
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